DC-506

1. Place seat of chair upside down.
2. Take base of chair and line up the eyelets on the base with the eyelets on the bottom of the seat.
3. Insert the given bolts into the eyelets loosely.
4. Once all bolts have been inserted into their hole tighten the bolts with the Allen wrench that is provided.  Do this in a diagonal manner.