DR71358 instructions

Place the table top upside down on the floor.

Unscrew the washer and nut from the thinner rod.

Screw the thinner rod into the table top.

Place the thicker rod over the thinner rod.

Place the base onto the thinner rod and thicker rod

Screw the washer and nut onto the thinner rod to hold the base.