INSTRUCTIONS FOR ITEM RT-412-BLACK

1 – Insert large o ring onto male end of silver leg, on all four legs

2 – Insert sliver legs into the black Y base so that all the holes line up and match

3 – Place black lock washers onto small black bolt and screw into all holes in the Y base

4 – Place small o ring onto foot and screw foot into the leg (do this for all four legs)

5 – Flip the base upside down

6 – Attach the black angle iron to the top of the leg so that the iron is flush with the top of the leg (do this for all four legs – use the large black bolts for this)

7 – Lay the table top facing down

8 – Flip the entire base over

9 – Insert sliver washer unto bolt and screw the angle iron into the table.

Flip table over and enjoy.